TUGAS 1. DASAR TEKNIK ELEKTRO

1. The hot resistance of a 250V filament lamp is 625  Ω Determine the current taken by the
    lamp and its power rating. 

2. Determine the resistance of a coil connectedto a 150Vsupply when a current of 
    (a) 75mA
    (b) 300 μA flows through it.


3. Determine the resistance of an electric fire which takes a current of 12A from a 240V
    supply. Find also the power rating of the fire and the energy used in 20 h.


4. Determine the power dissipated when a current of 10mA flows through an appliance
     having a resistance of 8 kΩ

5. 85.5 J of energy are converted into heat in 9 s. What power is dissipated? 
